#Title:Y8
#Author:SP2 Beta1
#Version:NOTHING DONE but to add extra parameters Need Data
#MODIF MAV-JP / STORE LIMITER / TO BE USED WITH ASSOCIATED WCD
#
# SIMULATION INPUT PANEL
#
# INPUT MASS AND GEOMETRIC PROPERTIES:
         30500  # Empty Weight (lbs)
          4000  # Reference Area
         10560  # Internal Fuel
#
#
# ANGLE OF ATTACK AND SIDESLIP LIMITS
            20  # AOA Max
            -5  # AOA Min
             5  # Beta Max
            -5  # Beta Min
             3  # Max G
            60  # Max Roll
           250  # Min Vcas
           650  # Max Vcas
           450  # Corner Vcas
            10  # Theta Max
             3  # Num Gear
# Gear X, Y, Z, Rng
          15.5             0             6           100
           150       -23.875             6           100
           150        23.875             6           100
#
# Physical data
            55  # CG Loc
           161  # Length
           185  # Span
            10  # Fus Radius
            20  # Tail Ht
#
# End of Airframe data
#
#
#
#     BASIC AERODYNAMIC COEFFICIENTS
#
#
#     MACH BREAKPOINTS
#
9   # Num MACH
             0           0.2           0.4           0.6
           0.8           0.9             1           1.1           1.2
#
#     ALPHA BREAKPOINTS
#
10   # Num Alpha
           -20           -10            -5             0
             5            10            15            20            25
            30
#
#     LIFT COEFFICIENT  CL
#
             1  # Table Multiplier
#
# Mach 0.00
       -0.8856       -0.6644       -0.2791        -0.025         0.365        0.7471
        1.1019        1.3764        1.5576        1.8158
#
# Mach 0.20
       -0.8856       -0.6644       -0.2791        -0.025         0.365        0.7471
        1.1019        1.3764        1.5576        1.8158
#
# Mach 0.40
       -0.8877       -0.6645         -0.28        -0.026         0.366         0.751
        1.1216        1.3787        1.5584        1.8179
#
# Mach 0.60
       -0.8878       -0.6646        -0.281       -0.0277         0.369        0.7554
        1.1265        1.3798        1.5589         1.818
#
# Mach 0.80
         -0.91        -0.685       -0.2956        -0.031        0.3987        0.7721
        1.1364        1.3987        1.5654        1.8223
#
# Mach 0.90
       -0.9542       -0.7086       -0.3276       -0.0442        0.4312        0.8021
        1.1455        1.4216        1.5877        1.8433
#
# Mach 1.00
       -0.9788         -0.71       -0.3332       -0.0466        0.4398        0.8099
        1.1502        1.4266        1.5986        1.8571
#
# Mach 1.10
       -0.9533       -0.6994       -0.3122       -0.0409        0.4221        0.7865
        1.1355        1.4176         1.562        1.8228
#
# Mach 1.20
       -0.9033       -0.6112       -0.2221       -0.0221        0.3088          0.71
        0.9065        1.3765        1.5001        1.7654
#
#     DRAG COEFFICIENT  CD
#
         0.526  # Table Multiplier
#
# Mach 0.00
        0.2674        0.2169        0.1031        0.0489        0.0386         0.082
        0.1843        0.3644        0.5829         0.871
#
# Mach 0.20
        0.2674        0.2169        0.1031        0.0489        0.0386         0.082
        0.1843        0.3644        0.5829         0.871
#
# Mach 0.40
        0.2674        0.2169        0.1031        0.0489        0.0386         0.082
        0.1843        0.3644        0.5829         0.871
#
# Mach 0.60
        0.2764        0.2213        0.1097         0.051          0.04        0.0877
        0.1902        0.3708        0.5954        0.8808
#
# Mach 0.80
        0.2802        0.2298        0.1106        0.0509        0.0412        0.0899
        0.1905        0.3732        0.5898          0.88
#
# Mach 0.90
        0.2904        0.2322        0.1209        0.0533        0.0567         0.091
        0.1987        0.3889        0.6008        0.8965
#
# Mach 1.00
        0.3304        0.2432        0.1541        0.0788        0.0986         0.123
        0.2253        0.4056        0.6243         0.911
#
# Mach 1.10
        0.3884        0.2601        0.1731        0.0809         0.105        0.1366
        0.2388        0.4176        0.6355         0.929
#
# Mach 1.20
         0.394        0.2679          0.18        0.0859          0.11        0.1401
          0.24        0.4215         0.641        0.9301
#
#     SIDE FORCE DERIVATIVE CY-BETA
#
             1  # Table Multiplier
#
# Mach 0.00
        -0.011       -0.0109       -0.0166       -0.0182       -0.0192       -0.0187
       -0.0163       -0.0176       -0.0164       -0.0158
#
# Mach 0.20
        -0.011       -0.0109       -0.0166       -0.0182       -0.0192       -0.0187
       -0.0163       -0.0176       -0.0164       -0.0158
#
# Mach 0.40
        -0.011       -0.0109       -0.0166       -0.0182       -0.0192       -0.0187
       -0.0163       -0.0176       -0.0164       -0.0158
#
# Mach 0.60
       -0.0115       -0.0112       -0.0172        -0.019       -0.0196       -0.0196
       -0.0168       -0.0178       -0.0167       -0.0161
#
# Mach 0.80
        -0.012       -0.0118        -0.018       -0.0195       -0.0197         -0.02
       -0.0174       -0.0182       -0.0171       -0.0168
#
# Mach 0.90
        -0.016       -0.0122        -0.021        -0.028       -0.0286         -0.03
        -0.025       -0.0267       -0.0223       -0.0215
#
# Mach 1.00
        -0.017       -0.0172        -0.027        -0.033        -0.035       -0.0333
       -0.0321       -0.0288       -0.0254       -0.0231
#
# Mach 1.10
       -0.0172       -0.0173       -0.0272       -0.0335       -0.0355       -0.0338
       -0.0326       -0.0292        -0.026        -0.024
#
# Mach 1.20
        -0.017       -0.0171        -0.026        -0.031        -0.032       -0.0321
       -0.0322       -0.0278       -0.0242       -0.0198
# End of Aero Data
#
#
# PROPULSION DATA
#
             2  # Thrust multiplier
             1  # Fuel Flow Multiplier
#
# MACH BREAKPOINTS
#
9   # Number of Mach Breaks
             0           0.2           0.4           0.6           0.8           0.9
             1           1.1           1.2
#
#     ALTITUDE BREAKPOINTS
#
6   # Number of Alt Break Points
             0          5000         10000         15000         35000         60000
#
#    THRST1 - THRUST AT IDLE (THROTL = 0.00)
#
# Alt 0
             0             0          -400         -1500         -3500         -4700         -4700         -4700         -4700
#
# Alt 5000
           300           300             0          -900         -2500         -3600         -3600         -3600         -3600
#
# Alt 10000
           500           500           100          -800         -1700         -2500         -2500         -2500         -2500
#
# Alt 15000
           800           800           700           100         -1000         -1700         -1700         -1700         -1700
#
# Alt 35000
           800           800           700           100         -1000         -1700         -1700         -1700         -1700
#
# Alt 60000
             0             0             0             0             0             0             0             0             0
#
#    THRST2 - THRUST AT MIL POWER (THROTL = 1.00)
#
# Alt 0
         15000         15000         16000         16000         17000         17000         17000         17000         17000
#
# Alt 5000
         12000         12000         13000         14000         15000         15000         15000         15000         15000
#
# Alt 10000
         10000         10000         11000         12000         13000         13000         13000         13000         13000
#
# Alt 15000
         10000         10000         10000         10000         11000         12000         12000         12000         12000
#
# Alt 35000
         10000         10000         10000         10000         11000         12000         12000         12000         12000
#
# Alt 60000
             0             0             0             0             0             0             0             0             0
#
#    THRST3 - THRUST AT FULL AB (THROTL = 1.05)
#
# Alt 0
         26000         26000         30000         32000         34000         34000         34000         34000         34000
#
# Alt 5000
         23000         23000         25000         26000         30000         32000         32000         32000         32000
#
# Alt 10000
         18000         18000         21000         23000         27000         30000         30000         30000         30000
#
# Alt 15000
         15000         15000         16000         19000         23000         26000         26000         26000         26000
#
# Alt 35000
         15000         15000         16000         19000         23000         23000         23000         23000         23000
#
# Alt 60000
             0             0             0             0             0             0             0             0             0
#
#    ROLL DATA
#
#
#    ALPHA BREAKPOINTS
6   # Num ALPHA
           -10             0            10            20            30            40
#
#     DYNAMIC PRESSURE BREAKPOINTS
#
7   # Num QBAR
             0           100           200           300           400           500
           600
#
#     RCMDMX - PEAK ROLL RATE
#
           0.4  # Table Multiplier
#
# ALPHA -10
            50            75            90           100           100           100           100
#
# ALPHA 0
            50            75            90           100           100           100           100
#
# ALPHA 10
            50            75            90           100           100           100           100
#
# ALPHA 20
            35            50            75            80            80            80            80
#
# ALPHA 30
            25            35            50            50            50            50            50
#
# ALPHA 40
           2.5            15            22            30            30            30            30
#
# End Of Roll Data
#
#
# LIMITERS
#
17   # Number of limiters
# Type Key Values
#
# Neg G Limiter
0 0            250            -3           100             0
# Pos G Limiter (Cat I)
3 1             15             9          20.4           7.3            25             1
# Roll Rate Limiter
0 2             15             1            29             0
# Yaw Alpha Limiter
0 3             14             1            26             0
# Yaw Roll Rate Limiter
0 4             20             1           360             0
# Cat III Command Type
0 5            100             7           420            15
# Cat III AOA Limiter
1 6             17
# Cat III Roll Rate Limiter
2 7            0.6
# Cat III Yaw Alpha Limiter
0 8              3             1            15             0
# Cat III Yaw Roll Rate Limiter
0 9             20             1           180             0
# Pitch and Yaw Control Damper
3 10              0           0.3            15          0.85            50             1
# Roll Control Damper
3 11              0           0.6            15          0.85            50             1
# Command Type
1 12             15
# Low Speed Omega
3 13           0.01           0.1            40           0.8            60             1
# Stores Drag
0 14            0.9       0.0001             1       0.000283
# Cat III Max Gs
1 16              6
# AOA Limiter
1 17             30
#
# End Of Limiters
#
#
#  ADDITIONAL DATA
#
normSpoolRate 0.7
abSpoolRate 0.4
jfsSpoolUpRate 15
jfsSpoolUpLimit 0.25
lightupSpoolRate 10
flameoutSpoolRate 35
jfsRechargeTime 60
jfsMinRechargeRpm 0.12
jfsSpinTime 240
mainGenRpm 0.63
stbyGenRpm 0.6
epuBurnTime 600
DeepStallEngineStall 0
engineDamageStopThreshold 15
engineDamageNoRestartThreshold 3
engineDamageHitThreshold 38
rollMomentum 1
pitchMomentum 1
yawMomentum 1
pitchElasticity 1
gearPitchFactor 0
rollGearGain 1
yawGearGain 1
pitchGearGain 1
sinkRate 15
tefMaxAngle 20
hasFlapperons 1
hasTef 2
CLtefFactor 0.05
CDtefFactor 0.05
tefNStages 2
tefTakeoff 0
tefRate 5
lefRate 5
hasLef 2
lefGround -2
lefMaxAngle 20
lefMaxMach 0.4
lefNStages 1
CDlefFactor 0
CDSPDBFactor 0.08
CDLDGFactor 0.06
flapGearRelative 1
maxFlapVcas 370
flapVcasRange 130
area2Span 0.0462
rudderMaxAngle 20
aileronMaxAngle 20
elevonMaxAngle 20
airbrakeMaxAngle 60
hasSwingWing 0
isComplex 0
landingAOA 12.5
dragChuteCd 0
dragChuteMaxSpeed 170
rollCouple -0.05
elevatorRoll 1
canopyMaxAngle 20
canopyRate 5
fuelFlowFactorNormal 180
fuelFlowFactorAb 444
minFuelFlow 1200
fuelFwdRes 0
fuelAftRes 0
fuelFwd1 0
fuelAft1 0
fuelWingAl 0
fuelWingFr 0
fuelFwdResRate 0
fuelAftResRate 0
fuelFwd1Rate 0
fuelAft1Rate 0
fuelWingAlRate 0
fuelWingFrRate 0
fuelClineRate 0
fuelWingExtRate 0
fuelMinFwd 400
fuelMinAft 250
nChaff 30
nFlare 60
gunLocation 2 -2 0
nEngines 1
engine1Location 0 0 0
engine2Location 0 0 0
engine3Location 0 0 0
engine4Location 0 0 0
engineSmokes 0
wingTipLocation 0 0 0
refuelLocation 0 0 0
hardpoint1Grp 0
hardpoint2Grp 0
hardpoint3Grp 0
hardpoint4Grp 0
hardpoint5Grp 0
hardpoint6Grp 0
hardpoint7Grp 0
hardpoint8Grp 0
hardpoint9Grp 0
hardpoint10Grp 0
hardpoint11Grp 0
hardpoint12Grp 0
hardpoint13Grp 0
hardpoint14Grp 0
hardpoint15Grp 0
hardpoint16Grp 0
sndExt 219
sndWind 33
sndAbInt 40
sndAbExt 224
sndEject 5
sndSpdBrakeStart 141
sndSpdBrakeLoop 140
sndSpdBrakeEnd 139
sndSpdBrakeWind 142
sndOverSpeed1 191
sndOverSpeed2 192
sndGunStart 25
sndGunLoop 26
sndGunEnd 27
sndBBPullup 68
sndBBBingo 66
sndBBWarning 63
sndBBCaution 64
sndBBChaffFlareLow 184
sndBBFlare 138
sndBBChaffFlare 183
sndBBChaffFlareOut 185
sndBBAltitude 65
sndBBLock 67
sndTouchDown 42
sndWheelBrakes 132
sndDragChute 218
sndLowSpeed 167
sndFlapStart 145
sndFlapLoop 144
sndFlapEnd 143
sndHookStart 195
sndHookLoop 194
sndHookEnd 193
sndGearCloseStart 147
sndGearCloseEnd 146
sndGearOpenStart 149
sndGearOpenEnd 150
sndGearLoop 148
rollLimitForAiInWP 30
flap2Nozzle 0
refuelSpeed 310
refuelAltitude 22500
decelDistance 1000
followRate 20
desiredClosureFactor 0.35
IL78Factor 0
longLeg 60
shortLeg 25
refuelRate 50
AIBoomDistance 50
BingoReturnDistance 50
jokerFactor 5
bingoFactor 5
fumesFactor 15
maxRippleCount 99
largePark 0
Has_TFR 0
PID_K 0.6
PID_KI 0
PID_KD 0.3
TFR_LimitMX 0
TFR_Corner 350
TFR_Gain 0.015
EVA_Gain 5
TFR_MaxRoll 20
TFR_SoftG 2
TFR_MedG 4
TFR_HardG 6
TFR_Clearance 20
SlowPercent 0
TFR_lookAhead 2000
EVA1_SoftFactor 0.6
EVA2_SoftFactor 0.4
EVA1_MedFactor 0.8
EVA2_MedFactor 0.6
EVA1_HardFactor 1.2
EVA2_HardFactor 0.9
TFR_GammaCorrMult 0.5
LantirnCameraX 10
LantirnCameraY 2
LantirnCameraZ 5
MinTGTMAR 0
MaxMARIdedStart 0
AddMARIded5k 0
AddMARIded18k 0
AddMARIded28k 0
AddMARIdedSpike 0
// Camera TopGun by Revientor
// left wing looking towards cockpit
TopGunCamera1 7 -20.3 -55.6 -2.5 0.0 10.0 0.0 60.0
// right of cockpit looking toward pilots
TopGunCamera2 7 63.4 -55.5 -2.5 0.0 120.0 0.0 60.0
// before air intake looking backwards to gear..
TopGunCamera3 7 50.0 -0.0 7.6 -2.0 -180.0 0.0 60.0
// placed near the gun (created by Revient0R), looking backward..
//TopGunCamera4
TopGunCamera4 7 146.1 0.0 -21.5 -13.0 180.0 0.0 47.0
#
# End of Additional
#

END OF DATA