#Title:AV8B
#Author:SP2 Beta1 Max Speed SL: 573 knots, Alt: 0.98 Mach
#Version:Engine 23,800 gross RR Pegasus 11.61 Engine
#MODIF MAV-JP / STORE LIMITER / TO BE USED WITH ASSOCIATED WCD
#
# SIMULATION INPUT PANEL
#
# INPUT MASS AND GEOMETRIC PROPERTIES:
         13968  # Empty Weight (lbs)
           230  # Reference Area
          7759  # Internal Fuel
#
#
# ANGLE OF ATTACK AND SIDESLIP LIMITS
            30  # AOA Max
           -10  # AOA Min
            20  # Beta Max
           -20  # Beta Min
             8  # Max G
           190  # Max Roll
           160  # Min Vcas
          1200  # Max Vcas
           450  # Corner Vcas
            70  # Theta Max
             3  # Num Gear
# Gear X, Y, Z, Rng
          13.3             0             7           100
          26.1            -2             7           100
          26.1             2             7           100
#
# Physical data
            23  # CG Loc
            46  # Length
            30  # Span
           3.3  # Fus Radius
            11  # Tail Ht
#
# End of Airframe data
#
#
#
#     BASIC AERODYNAMIC COEFFICIENTS
#
#
#     MACH BREAKPOINTS
#
3   # Num MACH
             0           0.6           0.9
#
#     ALPHA BREAKPOINTS
#
25   # Num Alpha
           -20           -10            -4            -2
             0             2             4             6             8
            10            12            14            16            18
            20            22            24            26            28
            30            32            34            36            38
            40
#
#     LIFT COEFFICIENT  CL
#
             1  # Table Multiplier
#
# Mach 0.00
       -0.8506        -0.629        -0.193       -0.0921          0.01          0.12
          0.23          0.39          0.51          0.63          0.79          0.92          1.05
        1.1598        1.2696       1.34208       1.41456       1.50244       1.60572         1.709
       1.74036       1.77172       1.78518       1.78074        1.7763
#
# Mach 0.60
        -0.859        -0.634      -0.19168    -0.0863692          0.02          0.16
          0.31          0.44           0.6          0.74          0.91           1.1       1.22532
       1.33024       1.43516       1.50184       1.56852       1.65324         1.756       1.85876
       1.90008        1.9414       1.96128       1.95972       1.95816
#
# Mach 0.90
         -0.89       -0.6444      -0.20672    -0.0939268          0.02          0.16
          0.31          0.44           0.6          0.74          0.91           1.1        1.2239
       1.33434       1.44478       1.51122       1.57766         1.662       1.76424       1.86648
       1.90868       1.95088       1.97286       1.97462       1.97638
#
#     DRAG COEFFICIENT  CD
#
       0.66666  # Table Multiplier
#
# Mach 0.00
       0.23872      0.188792     0.0657417      0.044424       0.02495        0.0246
       0.02575       0.03155         0.041        0.0545         0.083      0.122307      0.197831
      0.308463      0.419095      0.465894      0.512694      0.593005      0.706827      0.820653
      0.919147        1.0176       1.11768       1.21924        1.3208
#
# Mach 0.60
      0.202582      0.162766     0.0591655     0.0403947        0.0249        0.0248
       0.02795        0.0352          0.05         0.073       0.10557      0.137359      0.182121
      0.239854      0.297587       0.36603      0.434478      0.514553      0.606256       0.69796
        0.7738       0.84964      0.929873        1.0145       1.09912
#
# Mach 0.90
       0.22004      0.174062     0.0754547     0.0541996        0.0362        0.0362
       0.04335         0.057           0.1      0.112735      0.144872      0.177009      0.223129
      0.283233      0.343336      0.410296      0.477257      0.557457      0.650899       0.74434
      0.852507      0.960673       1.03873       1.08666        1.1346
#
#     SIDE FORCE DERIVATIVE CY-BETA
#
             1  # Table Multiplier
#
# Mach 0.00
        -0.011       -0.0109       -0.0166        -0.017       -0.0182        -0.019
       -0.0192       -0.0194       -0.0187       -0.0173        -0.017       -0.0163       -0.0169
       -0.0176       -0.0165       -0.0164       -0.0159       -0.0158       -0.0152       -0.0147
       -0.0143       -0.0141       -0.0139        -0.012        -0.009
#
# Mach 0.60
        -0.016       -0.0122        -0.017        -0.021        -0.023        -0.028
       -0.0283       -0.0286         -0.03       -0.0294        -0.025        -0.026       -0.0267
       -0.0253        -0.024       -0.0231       -0.0223       -0.0219       -0.0215       -0.0204
       -0.0197        -0.019       -0.0187       -0.0183       -0.0172
#
# Mach 0.90
        -0.016       -0.0122        -0.017        -0.021        -0.023        -0.028
       -0.0283       -0.0286         -0.03       -0.0294        -0.025        -0.026       -0.0267
       -0.0253        -0.024       -0.0231       -0.0223       -0.0219       -0.0215       -0.0204
       -0.0197        -0.019       -0.0187       -0.0183       -0.0172
# End of Aero Data
#
#
# PROPULSION DATA
#
             1  # Thrust multiplier
           0.8  # Fuel Flow Multiplier
#
# MACH BREAKPOINTS
#
7   # Number of Mach Breaks
             0           0.2           0.4           0.6           0.8             1
           1.2
#
#     ALTITUDE BREAKPOINTS
#
7   # Number of Alt Break Points
             0         10000         20000         30000         36000         40000
         50000
#
#    THRST1 - THRUST AT IDLE (THROTL = 0.00)
#
# Alt 0
             0          -800         -1700         -2200         -3300         -4000         -4900
#
# Alt 10000
             0          -400         -1100         -1650         -2250         -2800         -3450
#
# Alt 20000
             0          -370          -740         -1100         -1480         -1850         -2230
#
# Alt 30000
             0          -230          -450          -690          -920         -1150         -1380
#
# Alt 36000
             0          -160          -340          -500          -675          -850         -1000
#
# Alt 40000
             0          -140          -275          -415          -550          -690          -835
#
# Alt 50000
             0           -80          -170          -225          -345          -430          -515
#
#    THRST2 - THRUST AT MIL POWER (THROTL = 1.00)
#
# Alt 0
       16863.6         16116       16448.2       16863.6       16780.5         12000         10000
#
# Alt 10000
       11630.1       11131.6       11297.8       12377.7       14122.2         10000         10000
#
# Alt 20000
       7725.69        7393.4       7559.54       8224.12       9553.27          5000          5000
#
# Alt 30000
       4984.32       4818.17       4901.24       5399.67       6230.39          3000          3000
#
# Alt 36000
       3821.31       3655.16       3738.24       4070.52       4652.03          1500          1500
#
# Alt 40000
       3156.73       2990.59       3156.73       3322.88       3738.24          1200          1200
#
# Alt 50000
        2076.8       1993.73       1993.73        2076.8       2492.16           700           700
#
#    THRST3 - THRUST AT FULL AB (THROTL = 1.05)
#
# Alt 0
       16863.6         16116       16448.2       16863.6       16780.5         12000         10000
#
# Alt 10000
       11630.1       11131.6       11297.8       12377.7       14122.2         10000         10000
#
# Alt 20000
       7725.69        7393.4       7559.54       8224.12       9553.27          5000          5000
#
# Alt 30000
       4984.32       4818.17       4901.24       5399.67       6230.39          3000          3000
#
# Alt 36000
       3821.31       3655.16       3738.24       4070.52       4652.03          1500          1500
#
# Alt 40000
       3156.73       2990.59       3156.73       3322.88       3738.24          1200          1200
#
# Alt 50000
        2076.8       1993.73       1993.73        2076.8       2492.16           700           700
#
#    ROLL DATA
#
#
#    ALPHA BREAKPOINTS
7   # Num ALPHA
           -10             0            10            20            30            40            90
#
#     DYNAMIC PRESSURE BREAKPOINTS
#
7   # Num QBAR
             0           100           200           300           400           500
          2000
#
#     RCMDMX - PEAK ROLL RATE
#
             1  # Table Multiplier
#
# ALPHA -10
             0         56.82        113.64           125        147.73        147.73        136.36
#
# ALPHA 0
             0        159.09        215.91        227.27           250           250        238.64
#
# ALPHA 10
             0         56.82        113.64           125        147.73        147.73        136.36
#
# ALPHA 20
             0         11.36         22.73         34.09         45.45         45.45         45.45
#
# ALPHA 30
             0          5.68          5.68         17.05         28.41         28.41         22.73
#
# ALPHA 40
             0             0             0             0             0             0             0
#
# ALPHA 90

             0
             0
             0
             0
             0
             0
             0
#
# End Of Roll Data
#
#
# LIMITERS
#
17   # Number of limiters
# Type Key Values
#
# Neg G Limiter
0 0            250            -3           100             0
# Pos G Limiter (Cat I)
3 1             15             9          20.4           7.3            25             1
# Roll Rate Limiter
0 2             15             1            29             0
# Yaw Alpha Limiter
0 3             14             1            26             0
# Yaw Roll Rate Limiter
0 4             20             1           360             0
# Cat III Command Type
0 5            100             7           420            15
# Cat III AOA Limiter
1 6             17
# Cat III Roll Rate Limiter
2 7            0.6
# Cat III Yaw Alpha Limiter
0 8              3             1            15             0
# Cat III Yaw Roll Rate Limiter
0 9             20             1           180             0
# Pitch and Yaw Control Damper
3 10              0           0.3            15          0.85            50             1
# Roll Control Damper
3 11              0           0.6            15          0.85            50             1
# Command Type
1 12             25
# Low Speed Omega
3 13           0.01             1            40             1            60             1
# Stores Drag
0 14            0.9       0.0001             1       0.000283
# Cat III Max Gs
1 16              6
# AOA Limiter
1 17             30
#
# End Of Limiters
#
#
#  ADDITIONAL DATA
#
normSpoolRate 1.3
abSpoolRate 1.3
jfsSpoolUpRate 15
jfsSpoolUpLimit 0.25
lightupSpoolRate 10
flameoutSpoolRate 35
jfsRechargeTime 60
jfsMinRechargeRpm 0.12
jfsSpinTime 240
mainGenRpm 0.63
stbyGenRpm 0.6
epuBurnTime 600
DeepStallEngineStall 0
engineDamageStopThreshold 15
engineDamageNoRestartThreshold 3
engineDamageHitThreshold 42
rollMomentum 1.3
pitchMomentum 1.3
yawMomentum 1.3
pitchElasticity 1
gearPitchFactor 0
rollGearGain 1
yawGearGain 1
pitchGearGain 1
sinkRate 15
tefMaxAngle 50
hasFlapperons 0
hasTef 1
CLtefFactor 9.5
CDtefFactor 7.5
tefNStages 10
tefTakeoff 30
tefRate 3
lefRate 5
hasLef 0
lefGround 0
lefMaxAngle 0
lefMaxMach 0.4
lefNStages 0
CDlefFactor 0.04
CDSPDBFactor 0.08
CDLDGFactor 0.03
flapGearRelative 0
maxFlapVcas 280
flapVcasRange 180
area2Span 0.1304
rudderMaxAngle 20
aileronMaxAngle 20
elevonMaxAngle 20
airbrakeMaxAngle 60
hasSwingWing 0
isComplex 0
landingAOA 10
dragChuteCd 0
dragChuteMaxSpeed 170
rollCouple -0.05
elevatorRoll 1
canopyMaxAngle 20
canopyRate 5
fuelFlowFactorNormal 0.6
fuelFlowFactorAb 0.6
minFuelFlow 742
fuelFwdRes 0
fuelAftRes 0
fuelFwd1 0
fuelAft1 0
fuelWingAl 0
fuelWingFr 0
fuelFwdResRate 0
fuelAftResRate 0
fuelFwd1Rate 0
fuelAft1Rate 0
fuelWingAlRate 0
fuelWingFrRate 0
fuelClineRate 0
fuelWingExtRate 0
fuelMinFwd 400
fuelMinAft 250
nChaff 30
nFlare 60
gunLocation 2 -2 0
nEngines 1
engine1Location -20 0 0
engine2Location 0 0 0
engine3Location 0 0 0
engine4Location 0 0 0
engineSmokes 0
wingTipLocation -6.6 14 1.3
refuelLocation 0 0 0
hardpoint1Grp 0
hardpoint2Grp pylon-left
hardpoint3Grp pylon-left
hardpoint4Grp pylon-left
hardpoint5Grp 0
hardpoint6Grp pylon-right
hardpoint7Grp pylon-right
hardpoint8Grp pylon-right
hardpoint9Grp 0
hardpoint10Grp 0
hardpoint11Grp 0
hardpoint12Grp 0
hardpoint13Grp 0
hardpoint14Grp 0
hardpoint15Grp 0
hardpoint16Grp 0
sndExt 231
sndWind 33
sndAbInt 40
sndAbExt 231
sndEject 5
sndSpdBrakeStart 141
sndSpdBrakeLoop 140
sndSpdBrakeEnd 139
sndSpdBrakeWind 142
sndOverSpeed1 191
sndOverSpeed2 192
sndGunStart 25
sndGunLoop 26
sndGunEnd 27
sndBBPullup 68
sndBBBingo 66
sndBBWarning 63
sndBBCaution 64
sndBBChaffFlareLow 184
sndBBFlare 138
sndBBChaffFlare 183
sndBBChaffFlareOut 185
sndBBAltitude 65
sndBBLock 67
sndTouchDown 42
sndWheelBrakes 132
sndDragChute 218
sndLowSpeed 167
sndFlapStart 145
sndFlapLoop 144
sndFlapEnd 143
sndHookStart 195
sndHookLoop 194
sndHookEnd 193
sndGearCloseStart 147
sndGearCloseEnd 146
sndGearOpenStart 149
sndGearOpenEnd 150
sndGearLoop 148
rollLimitForAiInWP 60
flap2Nozzle 0
refuelSpeed 300
refuelAltitude 20000
decelDistance 5500
followRate 80
desiredClosureFactor 0.48
IL78Factor 22
longLeg 60
shortLeg 25
refuelRate 100
AIBoomDistance 10
BingoReturnDistance 50
jokerFactor 5.0
bingoFactor 5.0
fumesFactor 22.7
maxRippleCount 99
largePark 0
Has_TFR 0
PID_K 0.6
PID_KI 0
PID_KD 0.3
TFR_LimitMX 0
TFR_Corner 350
TFR_Gain 0.015
EVA_Gain 5
TFR_MaxRoll 20
TFR_SoftG 2
TFR_MedG 4
TFR_HardG 6
TFR_Clearance 20
SlowPercent 0
TFR_lookAhead 2000
EVA1_SoftFactor 0.6
EVA2_SoftFactor 0.4
EVA1_MedFactor 0.8
EVA2_MedFactor 0.6
EVA1_HardFactor 1.2
EVA2_HardFactor 0.9
TFR_GammaCorrMult 0.5
LantirnCameraX 10
LantirnCameraY 2
LantirnCameraZ 5
MinTGTMAR 0
MaxMARIdedStart 0
AddMARIded5k 0
AddMARIded18k 0
AddMARIded28k 0
AddMARIdedSpike 0
PilotEyePos 14.3 0 -1.5
// Camera TopGun by Revientor
// left wing looking towards cockpit
TopGunCamera1 7 -3.5 -17.1 -2.0 0.0 35.0 0.0 60.0
// right of cockpit looking toward pilots
TopGunCamera2 7 26.0 -23.1 -2.0 0.0 120.0 0.0 60.0
// before air intake looking backwards to gear..
TopGunCamera3 7 20.5 -0.0 7.3 13.0 -180.0 0.0 60.0
// placed near the gun (created by Revient0R), looking backward..
//TopGunCamera4
TopGunCamera4 7 56.0 0.0 -7.0 -13.0 180.0 0.0 47.0
#
# End of Additional
#

END OF DATA